{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["ＬＧＳ　ﾎﾞｰﾄﾞ"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"ＬＧＳ　ﾎﾞｰﾄﾞ","index":0,"n_rows":30,"n_cols":7,"rows_kept":30,"flags":["formulas_cached_only"]}
[]
[]
[null,null,"記号","名　　　　　　　   称","仕　　　　　　様","数　量","単位"]
[]
[]
[{"$nulls":3},"（仮称）ホテル計画  建設工事"]
[]
[]
[null,null,"記号","名　　　　　　　   称","仕　　　　　　様","数　量","単位"]
[]
[]
[null,null,"2","ボード工事"]
[]
[{"$nulls":3},"  （  外    部  ）"]
[{"$nulls":3},"軒裏","      Ｔ"]
[{"$nulls":3},"ケイ酸カルシウム板","     6.0  軽鉄面･塗装下",4.8,"m2"]
[{"$nulls":3},"軒裏","      Ｔ"]
[{"$nulls":3},"ケイ酸カルシウム板","     6.0  軽鉄面･吹付下",{"v":2,"d":"2.0"},"m2"]
[{"$nulls":3},"バルコニー  軒裏","      Ｔ"]
[{"$nulls":3},"ケイ酸カルシウム板","     6.0  軽鉄面･吹付下",40.3,"m2"]
[{"$nulls":3},"バルコニー  折上天井","      Ｔ"]
[{"$nulls":3},"ケイ酸カルシウム板","     6.0  軽鉄面･吹付下",13.4,"m2"]
[]
[]
[{"$nulls":3},"天井裏","      Ｔ"]
[{"$nulls":3},"グラスウール敷込","      50  24Kg品",4.8,"m2"]
[]
[]
[{"$nulls":3},"ルーフテラス　軒天","      Ｔ"]
[{"$nulls":3},"ケイ酸カルシウム板","     6.0  軽鉄面･吹付下",48.7,"㎥"]